# Black Magic Probe
# there are two connections, one for GDB and one for UART debugging
# copy this to /etc/udev/rules.d/99-blackmagic.rules
# and run /usr/sbin/udevadm control --reload-rules
SUBSYSTEM=="tty", ACTION=="add", ATTRS{interface}=="Black Magic GDB Server", SYMLINK+="ttyBmpGdb"
SUBSYSTEM=="tty", ACTION=="add", ATTRS{interface}=="Black Magic UART Port", SYMLINK+="ttyBmpTarg"
SUBSYSTEM=="usb", ENV{DEVTYPE}=="usb_device", ATTR{idVendor}=="1d50", ATTR{idProduct}=="6017", MODE="0666"
SUBSYSTEM=="usb", ENV{DEVTYPE}=="usb_device", ATTR{idVendor}=="1d50", ATTR{idProduct}=="6018", MODE="0666"
